
**How to upgrade software for S-928 STB by using RS-232**

* 1. Your STB should be off and connected to your PC by using RS-232 serial cable.
  2. At first, run the program “Upgrade.exe” in your PC. And you can see the following pop-up screen.



* 1. Select the correct COM Port in your PC. by clicking No. # 1 in the above picture.
  2. Choose the software that you want download by clicking No. # 2 in the above picture.
  3. Click “Start”.
  4. Turn on your STB. And if your STB and PC are correctly connected by RS-232 cable The upgrade will start. (Please wait until it is completely finished.)

***Please do not turns off STB while progressing of the software downloading.***

* 1. When the following pop message displays, the upgrade is complete. And then, the receiver will be rebooted automatically.

